
#source
    
    A - B - C;
    A - B * C;

#bytecode
    
    PUSHVAR "A";
    PUSHVAR "B";
    SUB;
    PUSHVAR "C";
    SUB;
    POP 1;

    PUSHVAR "A";
    PUSHVAR "B";
    PUSHVAR "C";
    MUL;
    SUB;
    POP 1;

    EXIT;